# DE-Nano FPGA Board Configuration

## Pin Assignments:

- CLOCK
- LED
- KEY
- SW
- SDRAM
- EPCS
- Accelerometer and EEPROM
- ADC
- 2x13 GPIO Header
- GPIO_0
- GPIO_1

## Pin Assignment Table:

##

CLOCK
Name | Location | Direction | Standard
--- | --- | --- | ---
CLOCK_50 | R8 | input | 3.3-V LVTTL

##

LED
Name | Location | Direction | Standard
--- | --- | --- | ---
LED[0] | A15 | output | 3.3-V LVTTL
LED[1] | A13 | output | 3.3-V LVTTL
LED[2] | B13 | output | 3.3-V LVTTL
LED[3] | A11 | output | 3.3-V LVTTL
LED[4] | D1 | output | 3.3-V LVTTL
LED[5] | F3 | output | 3.3-V LVTTL
LED[6] | B1 | output | 3.3-V LVTTL
LED[7] | L3 | output | 3.3-V LVTTL

##

KEY
Name | Location | Direction | Standard
--- | --- | --- | ---
KEY[0] | J15 | input | 3.3-V LVTTL
KEY[1] | E1 | input | 3.3-V LVTTL

##

SW
Name | Location | Direction | Standard
--- | --- | --- | ---
SW[0] | M1 | input | 3.3-V LVTTL
SW[1] | T8 | input | 3.3-V LVTTL
SW[2] | B9 | input | 3.3-V LVTTL
SW[3] | M15 | input | 3.3-V LVTTL

##

SDRAM
Name | Location | Direction | Standard
--- | --- | --- | ---
DRAM_BA[0] | M7 | output | 3.3-V LVTTL
DRAM_BA[1] | M6 | output | 3.3-V LVTTL
DRAM_DQM[0] | R6 | output | 3.3-V LVTTL
DRAM_DQM[1] | T5 | output | 3.3-V LVTTL
DRAM_RAS_N | L2 | output | 3.3-V LVTTL
DRAM_CAS_N | L1 | output | 3.3-V LVTTL
DRAM_CKE | L7 | output | 3.3-V LVTTL
DRAM_CLK | R4 | output | 3.3-V LVTTL
DRAM_WE_N | C2 | output | 3.3-V LVTTL
DRAM_CS_N | P6 | output | 3.3-V LVTTL
DRAM_DQ[0] | G2 | inout | 3.3-V LVTTL
DRAM_DQ[1] | G1 | inout | 3.3-V LVTTL
DRAM_DQ[2] | L8 | inout | 3.3-V LVTTL
DRAM_DQ[3] | K5 | inout | 3.3-V LVTTL
DRAM_DQ[4] | K2 | inout | 3.3-V LVTTL
DRAM_DQ[5] | J2 | inout | 3.3-V LVTTL
DRAM_DQ[6] | J1 | inout | 3.3-V LVTTL
DRAM_DQ[7] | R7 | inout | 3.3-V LVTTL
DRAM_DQ[8] | T4 | inout | 3.3-V LVTTL
DRAM_DQ[9] | T2 | inout | 3.3-V LVTTL
DRAM_DQ[10] | T3 | inout | 3.3-V LVTTL
DRAM_DQ[11] | R3 | inout | 3.3-V LVTTL
DRAM_DQ[12] | R5 | inout | 3.3-V LVTTL
DRAM_DQ[13] | P3 | inout | 3.3-V LVTTL
DRAM_DQ[14] | N3 | inout | 3.3-V LVTTL
DRAM_DQ[15] | K1 | inout | 3.3-V LVTTL
DRAM_ADDR[0] | P2 | output | 3.3-V LVTTL
DRAM_ADDR[1] | N5 | output | 3.3-V LVTTL
DRAM_ADDR[2] | N6 | output | 3.3-V LVTTL
DRAM_ADDR[3] | M8 | output | 3.3-V LVTTL
DRAM_ADDR[4] | P8 | output | 3.3-V LVTTL
DRAM_ADDR[5] | T7 | output | 3.3-V LVTTL
DRAM_ADDR[6] | N8 | output | 3.3-V LVTTL
DRAM_ADDR[7] | T6 | output | 3.3-V LVTTL
DRAM_ADDR[8] | R1 | output | 3.3-V LVTTL
DRAM_ADDR[9] | P1 | output | 3.3-V LVTTL
DRAM_ADDR[10] | N2 | output | 3.3-V LVTTL
DRAM_ADDR[11] | N1 | output | 3.3-V LVTTL
DRAM_ADDR[12] | L4 | output | 3.3-V LVTTL

##

EPCS
Name | Location | Direction | Standard
--- | --- | --- | ---
EPCS_DATA0 | H2 | input | 3.3-V LVTTL
EPCS_DCLK | H1 | output | 3.3-V LVTTL
EPCS_NCSO | D2 | output | 3.3-V LVTTL
EPCS_ASDO | C1 | output | 3.3-V LVTTL

##

Accelerometer and EEPROM
Name | Location | Direction | Standard
--- | --- | --- | ---
I2C_SCLK | F2 | output | 3.3-V LVTTL
I2C_SDAT | F1 | inout | 3.3-V LVTTL
G_SENSOR_CS_N | G5 | output | 3.3-V LVTTL
G_SENSOR_INT | M2 | input | 3.3-V LVTTL

##

ADC
Name | Location | Direction | Standard
--- | --- | --- | ---
ADC_CS_N | A10 | output | 3.3-V LVTTL
ADC_SADDR | B10 | output | 3.3-V LVTTL
ADC_SCLK | B14 | output | 3.3-V LVTTL
ADC_SDAT | A9 | input | 3.3-V LVTTL

##

2x13 GPIO Header
Name | Location | Direction | Standard
--- | --- | --- | ---
GPIO_2[0] | A14 | inout | 3.3-V LVTTL
GPIO_2[1] | B16 | inout | 3.3-V LVTTL
GPIO_2[2] | C14 | inout | 3.3-V LVTTL
GPIO_2[3] | C16 | inout | 3.3-V LVTTL
GPIO_2[4] | C15 | inout | 3.3-V LVTTL
GPIO_2[5] | D16 | inout | 3.3-V LVTTL
GPIO_2[6] | D15 | inout | 3.3-V LVTTL
GPIO_2[7] | D14 | inout | 3.3-V LVTTL
GPIO_2[8] | F15 | inout | 3.3-V LVTTL
GPIO_2[9] | F16 | inout | 3.3-V LVTTL
GPIO_2[10] | F14 | inout | 3.3-V LVTTL
GPIO_2[11] | G16 | inout | 3.3-V LVTTL
GPIO_2[12] | G15 | inout | 3.3-V LVTTL
GPIO_2_IN[0] | E15 | input | 3.3-V LVTTL
GPIO_2_IN[1] | E16 | input | 3.3-V LVTTL
GPIO_2_IN[2] | M16 | input | 3.3-V LVTTL

##

GPIO_0 connect to GPIO Default
Name | Location | Direction | Standard | GPIO Pin Index
--- | --- | --- | --- | ---
GPIO_0_IN[0] | A8 | input | 3.3-V LVTTL | 1
GPIO_0[0] | D3 | inout | 3.3-V LVTTL | 2
GPIO_0_IN[1] | B8 | input | 3.3-V LVTTL | 3
GPIO_0[1] | C3 | inout | 3.3-V LVTTL | 4
GPIO_0[2] | A2 | inout | 3.3-V LVTTL | 5
GPIO_0[3] | A3 | inout | 3.3-V LVTTL | 6
GPIO_0[4] | B3 | inout | 3.3-V LVTTL | 7
GPIO_0[5] | B4 | inout | 3.3-V LVTTL | 8
GPIO_0[6] | A4 | inout | 3.3-V LVTTL | 9
GPIO_0[7] | B5 | inout | 3.3-V LVTTL | 10
GPIO_0[8] | A5 | inout | 3.3-V LVTTL | 13
GPIO_0[9] | D5 | inout | 3.3-V LVTTL | 14
GPIO_0[10] | B6 | inout | 3.3-V LVTTL | 15
GPIO_0[11] | A6 | inout | 3.3-V LVTTL | 16
GPIO_0[12] | B7 | inout | 3.3-V LVTTL | 17
GPIO_0[13] | D6 | inout | 3.3-V LVTTL | 18
GPIO_0[14] | A7 | inout | 3.3-V LVTTL | 19
GPIO_0[15] | C6 | inout | 3.3-V LVTTL | 20
GPIO_0[16] | C8 | inout | 3.3-V LVTTL | 21
GPIO_0[17] | E6 | inout | 3.3-V LVTTL | 22
GPIO_0[18] | E7 | inout | 3.3-V LVTTL | 23
GPIO_0[19] | D8 | inout | 3.3-V LVTTL | 24
GPIO_0[20] | E8 | inout | 3.3-V LVTTL | 25
GPIO_0[21] | F8 | inout | 3.3-V LVTTL | 26
GPIO_0[22] | F9 | inout | 3.3-V LVTTL | 27
GPIO_0[23] | E9 | inout | 3.3-V LVTTL | 28
GPIO_0[24] | C9 | inout | 3.3-V LVTTL | 31
GPIO_0[25] | D9 | inout | 3.3-V LVTTL | 32
GPIO_0[26] | E11 | inout | 3.3-V LVTTL | 33
GPIO_0[27] | E10 | inout | 3.3-V LVTTL | 34
GPIO_0[28] | C11 | inout | 3.3-V LVTTL | 35
GPIO_0[29] | B11 | inout | 3.3-V LVTTL | 36
GPIO_0[30] | A12 | inout | 3.3-V LVTTL | 37
GPIO_0[31] | D11 | inout | 3.3-V LVTTL | 38
GPIO_0[32] | D12 | inout | 3.3-V LVTTL | 39
GPIO_0[33] | B12 | inout | 3.3-V LVTTL | 40

##

GPIO_1 connect to GPIO Default
Name | Location | Direction | Standard | GPIO Pin Index
--- | --- | --- | --- | ---
GPIO_1_IN[0] | T9 | input | 3.3-V LVTTL | 1
GPIO_1[0] | F13 | inout | 3.3-V LVTTL | 2
GPIO_1_IN[1] | R9 | input | 3.3-V LVTTL | 3
GPIO_1[1] | T15 | inout | 3.3-V LVTTL | 4
GPIO_1[2] | T14 | inout | 3.3-V LVTTL | 5
GPIO_1[3] | T13 | inout | 3.3-V LVTTL | 6
GPIO_1[4] | R13 | inout | 3.3-V LVTTL | 7
GPIO_1[5] | T12 | inout | 3.3-V LVTTL | 8
GPIO_1[6] | R12 | inout | 3.3-V LVTTL | 9
GPIO_1[7] | T11 | inout | 3.3-V LVTTL | 10
GPIO_1[8] | T10 | inout | 3.3-V LVTTL | 13
GPIO_1[9] | R11 | inout | 3.3-V LVTTL | 14
GPIO_1[10] | P11 | inout | 3.3-V LVTTL | 15
GPIO_1[11] | R10 | inout | 3.3-V LVTTL | 16
GPIO_1[12] | N12 | inout | 3.3-V LVTTL | 17
GPIO_1[13] | P9 | inout | 3.3-V LVTTL | 18
GPIO_1[14] | N9 | inout | 3.3-V LVTTL | 19
GPIO_1[15] | N11 | inout | 3.3-V LVTTL | 20
GPIO_1[16] | L16 | inout | 3.3-V LVTTL | 21
GPIO_1[17] | K16 | inout | 3.3-V LVTTL | 22
GPIO_1[18] | R16 | inout | 3.3-V LVTTL | 23
GPIO_1[19] | L15 | inout | 3.3-V LVTTL | 24
GPIO_1[20] | P15 | inout | 3.3-V LVTTL | 25
GPIO_1[21] | P16 | inout | 3.3-V LVTTL | 26
GPIO_1[22] | R14 | inout | 3.3-V LVTTL | 27
GPIO_1[23] | N16 | inout | 3.3-V LVTTL | 28
GPIO_1[24] | N15 | inout | 3.3-V LVTTL | 31
GPIO_1[25] | P14 | inout | 3.3-V LVTTL | 32
GPIO_1[26] | L14 | inout | 3.3-V LVTTL | 33
GPIO_1[27] | N14 | inout | 3.3-V LVTTL | 34
GPIO_1[28] | M10 | inout | 3.3-V LVTTL | 35
GPIO_1[29] | L13 | inout | 3.3-V LVTTL | 36
GPIO_1[30] | J16 | inout | 3.3-V LVTTL | 37
GPIO_1[31] | K15 | inout | 3.3-V LVTTL | 38
GPIO_1[32] | J13 | inout | 3.3-V LVTTL | 39
GPIO_1[33] | J14 | inout | 3.3-V LVTTL | 40