# DE-Nano FPGA Board Configuration

## Pin Assignments:

- CLOCK
- LED
- KEY
- SW
- EEPROM

## Pin Assignment Table:

##

CLOCK
Name | Location | Direction | Standard
--- | --- | --- | ---
CLOCK_50 | R8 | input | 3.3-V LVTTL

##

LED
Name | Location | Direction | Standard
--- | --- | --- | ---
LED[0] | A15 | output | 3.3-V LVTTL
LED[1] | A13 | output | 3.3-V LVTTL
LED[2] | B13 | output | 3.3-V LVTTL
LED[3] | A11 | output | 3.3-V LVTTL
LED[4] | D1 | output | 3.3-V LVTTL
LED[5] | F3 | output | 3.3-V LVTTL
LED[6] | B1 | output | 3.3-V LVTTL
LED[7] | L3 | output | 3.3-V LVTTL

##

KEY
Name | Location | Direction | Standard
--- | --- | --- | ---
KEY[0] | J15 | input | 3.3-V LVTTL
KEY[1] | E1 | input | 3.3-V LVTTL

##

SW
Name | Location | Direction | Standard
--- | --- | --- | ---
SW[0] | M1 | input | 3.3-V LVTTL
SW[1] | T8 | input | 3.3-V LVTTL
SW[2] | B9 | input | 3.3-V LVTTL
SW[3] | M15 | input | 3.3-V LVTTL

##

EEPROM
Name | Location | Direction | Standard
--- | --- | --- | ---
I2C_SCLK | F2 | output | 3.3-V LVTTL
I2C_SDAT | F1 | inout | 3.3-V LVTTL